IC‑7300 Rig Control – Program Tips

Important: Keep all required files in the same folder as the program. The following files must be in the same directory as ic7300RigControlV1.exe:
• ic7300RigControlV
1.exe
• rig_defaults.json
• rig_log.csv
• rig_memories.json

You may place the shortcut 'Shortcut_ic7300RigControlV1' on your desktop if you want easy access to the program.

Setting the Correct COM Port

If your IC‑7300 radio is using a COM port other than COM3, you must update the program settings.
1. Start the program.
2. Change the COM port to match the port assigned to your radio.
3. Click the 'Set Defaults' button.
4. Close the program.
5. Restart the program so the changes take effect.
Changing Memory Presets
You can modify any of the memory presets.
1. Click on the preset slot you want to change.
2. Modify the frequency, mode, or other settings.
3. Click 'Save PRESET – Slot' to store the changes.
Changing Default Startup Values
If you want the program to start with specific values, change the settings you want and then click the 'Set Defaults' button at the top of the program.
